流媒体服务器使用标准的RTSP，RTP/RTCP协议，传送H264视频数据

请求格式如下

会话编号,请求类型,设备编号,通道号,码流类型,录像标识,保留字段

会话编号：为客户端的会话信息，暂时可以为空

请求类型：12545

设备编号：车辆的编号信息

通道号：从0开始

码流类型：1，表示子码流

录像标识：0，暂时无效

保留标识：0，暂时无效

将数据按协议组装后进行Base64编码

请求示例：

,12545,10000,0,1,0,0

请求含义如下：会话号为空，请求类型为12545，设备编号为10000，通道0，码流1，录像标识0，保留标识0

进行base64编码后，数据为：LDEyNTQ1LDEwMDAwLDAsMSwwLDA=

则请求的URL为 rtsp://192.168.8.12:8504/LDEyNTQ1LDEwMDAwLDAsMSwwLDA=

192.168.8.12为流媒体服务器的访问地址，8504为流媒体服务器的默认访问端口

,12545,180305111,0,0,0,0

493B87651F1848C0A363F9A544E0D39E,3,31304,2,0,0,0

,12545,31304,2,0,0,0

LDEyNTQ1LDE4MDMwNTExMSwwLDAsMCww

493B87651F1848C0A363F9A544E0D39E,3,31304,2,0,0,0 513F19776EE34035BDC0E8F05F4F8CED,3,31279,1,0,0,0 513F19776EE34035BDC0E8F05F4F8CED,3,31279,1,0,0,0

513F19776EE34035BDC0E8F05F4F8CED,3,31279,1,0,0,0

513F19776EE34035BDC0E8F05F4F8CED,3,31304,2,0,0,0

LDEyNTQ1LDMxMzA0LDIsMCwwLDA=

LDEyNTQ1LDMxMjc5LDEsMCwwLDA=

LDEyNTQ1LDMxMzA0LDIsMCwwLDA=

LDEyNTQ1LDMxMjc5LDEsMCwwLDA=

,12545,31279,1,0,0,0 LDEyNTQ1LDMxMjc5LDEsMCwwLDA=

,12545,31304,2,0,0,0 LDEyNTQ1LDMxMzA0LDIsMCwwLDA=

,12545,31279,1,0,0,0

2018-06-04 14:41:33, INFO, client\_ivs\_gateway.cpp,450: receive get media url req,url:000c29627a21-000c29627a211180000001-000c29627a211310000009-000c29627a210000009

2018-06-04 14:41:33, INFO, client\_ivs\_gateway.cpp,813: receive get media url rsp,result:0, url:rtsp://58.240.131.60:554/2268/rtsp://218.90.198.19:6604/LDEyNTQ1LDMxMzA0LDIsMCwwLDA=?BitRate=2048;FrameRate=25;IFrame=100;DmgType=2270

LDEyNTQ1LDMxMzA0LDIsMCwwLDA=

LDEyNTQ1LDMxMjc5LDEsMCwwLDA=

000c29627a211310000009 、、

LDEyNTQ1LDMxMjc5LDEsMCwwLDA=

LDEyNTQ1LDMxMzA0LDIsMCwwLDA=

,12545,31279,1,0,0,0

LDEyNTQ1LDMxMjc5LDEsMCwwLDA=

LDEyNTQ1LDMxMjM2LDEsMCwwLDA=

,12545,31304,2,0,0,0

,12545,31279,1,0,0,0